INSTALLATION NOTE

Product: **VOLTECH ISC-3040 MAXIMUM INPUT RATINGS;**

**PV Input Power: 360 Watts maximum on a 12 Volt Battery System**

**PV “ “ : 720 Watts maximum on a 24 Volt Battery System**

**PV Input Voltage: 65 Volts (max)**

This refers to the actual Open Circuit Voltage (**VoC**) of the PV Panel(s) as connected,

***Not*** the approximate figure of Maximum Power Voltage (Vmp).

Connecting the unit with an Input above 65V **will** damage the Controller & possibly other components of the PV system. This would be considered abuse & therefore not be covered by Warranty. We would suggest a safe operating limit of around 55 Volts (VoC).